- Resend activation?
- Lost password?
- Register
- Remember Me?

+ Post New Thread + Reply to Thread
Results 1 to 3 of 3

# Thread: developing 8 to 256 bit decoder

- ###### LinkBack

  - LinkBack URL
  - About LinkBacks
  - Bookmark & Share
  - Digg this Thread!
  - Add Thread to del.icio.us
  - Bookmark in Technorati
  - Tweet this thread

- ###### Thread Tools

  - Show Printable Version
  - Download This Thread
  - Subscribe to this Thread…

- ###### Search Thread

  - Advanced Search

1. 25-09-06, 12:48 #1
   karthyekrajhaa
   Newbie level 3

   Join Date
     Sep 2006
   Posts
     3
   Helped
     0 / 0
   Points
     754
   Level
     6

   ## decode 256 bit

   > will u help me in developing 8 to 256 bit decoder using 3 to 8 bit decoder circuits?

   Reply With Quote

- Advertising

2. 25-09-06, 17:17 #2
   nsit1234
   Newbie level 6

   Join Date
     May 2006
   Posts
     13
   Helped
     0 / 0
   Points
     996
   Level
     7

   ## 8 zu 256 decoder

   > u can make it in many ways
   > for that u have to know what is internal structure of the decoder
   > means in 3 to 8 bit decoder consists of 8 no.s of 3-input and gates or nand gates and 3 inverter gates
   > and what u want to do ,it needs 256+8 inputs
   > and u have to specify which types of other gates(two i/p or 3 i/ps and gates or nand gates)
   > etc. u need then u can make it
   > first tell me with what gates,decoders etc. u need to make that ckt. or u need to make the ckt. using only 3to8 decoders and how much no.s of that?????

   Reply With Quote

- Advertising

3. 25-09-06, 18:18 #3
   newelltech
   Full Member level 4

   Join Date
     Aug 2006
   Posts
     216
   Helped
     32 / 32
   Points
     2,383
   Level
     11

   ## 256 bit decoder

   > There is really only one way to do this assuming your decoder is standard and has 3 select pins and one enable pin.
   > Work backwards and start with the output. You will need 32 decoders to produce 256 outputs. Each of these decoders will use 3 bits of your 8 bit input, say I0,I1 and I2.
   > Next you will need to control the enable pins of your 32 decoders. For this you will need 4 more decoders. Each of these decoders will use 3 more bits of your 8 bit input, I3, I4 and I5. The outputs of these 4 decoders will give you 32 enable controls.
   > Finally you will need to control the enable pins of your group of 4 decoders. For this you will need 1 more decoder. This decoder will use the last 2 bits of your 8 bit input, I6 and I7 and the third input selector for this decoder will just be grounded. The outputs of this decoder will give you 4 outputs which will control the enable pins in the group of 4 decoders.
   > You will need to check how your enable pin works. It may set all the outputs to 0 which is what you want. If it tri-states the outputs, then you will have to add pull-down resistors if you're using CMOS logic. If so you can use the resistor packs that have 8 resistors in a dil package.

   1 members found this post helpful.
   Reply With Quote

+ Post New Thread + Reply to Thread
« How many kinds of reference circuits are there? | diff in 8086 & 8088 »

#### Similar Threads

1. ###### After developing what to do?how? (5)

2. ###### Gemini-4 Encoder-Decoder: error with the decoder (0)

3. ###### help in developing an algorithm (1)

4. ###### Developing an AC/DC Converter (3)

5. ###### Help me with developing a CAN protocol kit (0)